Date: 19/05/2021

Experiment: Recirculation of Helios devices at level 5

Description:

* Only limited sensors are used in this study as the point of interest is the Recirculation not the air change efficiency
* 2L sensor is in the ventilation device
* 3b at the centre, 1c, 3L\_Ku, 2e and 2d were working
* 3d measured outdoor which is on the top of test stand. 2a\_50 is inside the centre of outdoor chamber
* 3a\_50 is turning on and is somewhere, we suspected that it is in the outlet of the indoor chamber. But it does not appear to be the case
* Volume of the push-pull devices is at level 5

|  |  |  |
| --- | --- | --- |
| Time | Incident | Remarks |
| 17:25 | All setup is ready and the CO2 is filled in the indoor chamber |  |
| 18:01 | The setup is ready to start the experiment  The caps were open on the ventilation devices |  |
| 18:21 | Experiment concluded |  |
|  |  |  |